**9-6-18 Training – Radiogram End-of-text & Signature**

***Radiogram Training – End of Text & Signature - - -***

* After the text has been sent, say “BREAK FOR SIGNATURE”…
  + Note that more experienced traffic handlers just say “BREAK” at this poing
* …and immediately send the signature of the person sending the message
  + Send the Name and Call Sign (if the sender is a ham)
  + The signature may not be the same person as the ham originating the message!  He may be sending the message for someone else.
* Sometimes the signature includes a reply-to note (a “Service Note”)
  + “DL4FN via KW1U”
* After sending the signature, say “END” and the number of messages remaining to be sent – for example, if it’s only 1 message, say “END, NO MORE”.
  + If you’re sending several messages – say 3 messages – then say “END, 2 MORE”, “END, 1 MORE”, etc., until “END, NO MORE”
* After the “END” comment (“END, NO MORE” or whatever), just stop transmitting.  The “END” comment is the trigger for the receiving station to respond with either…
  + “ROGER” (or “ROGER, ROGER, ROGER if conditions are bad) or…
  + …ask for fills, clarification, or corrections.